|  |  |
| --- | --- |
| **This OCS…** | **To a PC (DTE)** |
| **Signal** | **RJ-45** | **9-pin D** | **Signal** |
| **RXD** | 8 | 2 | **RXD** |
| **TXD** | 7 | 3 | **TXD** |
| **GND** | 6 | 5 | **GND** |
|  |   | *Short pins 4 & 6 on 9-pin PC side for official programming cable* |
|   |   |
|   |   |